Preparing NEX camera for a dive

- set ISO to 400

- set LCD brightness to manual-max

- set focus mode to autofocus

- set focus-point selection mode to centre-spot

- set autofocus mode to AF-single

- switch AF illuminator off

- switch stabilizer on

- set shooting mode to Program

- set exposure compensation to -0.7

- load new memory card and format it

- load a new battery

- put a FLD filter on the lens

- set focal length to ~20mm

--------

- put silica-gel packs into the housing

- blow the dust off the housing

- close the housing